**Format Proposal from C. Wemple – 19 May 2014**

**File 2 Scattering Radius for LRF=7**

Proposed new evaluations for ENDF/B-VII R2 have indicated one remaining inconsistency in the resonance formats for the scattering radius, AP. After the revision to Section 2.2.1.2 from the November 2012 CSEWG meeting, only the limited R-matrix treatment (LRF=7) lacks a specification for AP in the formats. To bring this in line with the other resonance formats, a change is proposed for the first CONT record in Section 2.2.1.6.

Present version: **[MAT,2,151/ 0.0, 0.0, IFG, KRM, NJS, KRL ]CONT**

Proposed revision: **[MAT,2,151/ SPI, AP, IFG, KRM, NJS, KRL ]CONT**

This will make the initial CONT record in all resonance formats consistent.